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Filler Panel Request Form

	Date:
	
	Job name:
	

	Ship to:
	
	City, State:
	

	Attn:
	
	
	

	Address:
	
	Ordered by:
	

	City/St/Zip:
	
	Phone:
	

	Phone:
	
	email:
	

	email:
	
	DSL/Case ID#:
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	Total Quantity of enMotion® or Pacific Blue Ultra® Recessed panels needed.

	
	Total Quantity of enMotion® FLEX panels needed. 

	How to measure for a filler panel:

	View enMotion Recessed measuring instructions at: http://youtu.be/PsnyXddyUEw

	Flex Recessed measuring/install: https://www.youtube.com/watch?v=ui0BF58uFTI

	WIDTH:
	
	Outside
	Outside edge to Outside edge (closest 1/8”)

	WIDTH:
	
	Inside
	Cavity Inside left to Inside right (closest 1/8”)

	HEIGHT:
	
	Outside
	Outside edge to bottom of paper tray

	HEIGHT:
	
	Inside
	Cavity Inside to bottom of paper tray

	DEPTH:
	
	
	


														


ORDER
	Quantity
	Panel Requested
	Width
	Height Range
	Panel Style

	
	ER or PBUR: 57445: OM-22
	17 3/8”
	16” to 22”
	Outside Mount (preferred)

	
	ER or PBUR: 57443: IN-22
	15 1/8” to 15 ¼”
	20” to 22”
	Inside Mount

	
	ER or PBUR 57442: IN-20
	15 1/8” to 15 ¼”
	18” to 20”
	Inside Mount

	
	FLEX: 57745: OM-24.5
	17 3/8”
	18” to 24 1/2”
	Outside Mount (preferred)

	
	FLEX: 57743: IN-24.5
	15 1/8” to 15 ¼”
	20” to 24 1/2”
	Inside Mount

	Common Custom Panels

	
	ER or PBUR: OM-Contour
	17 5/8”
	16” to 22”
	Outside Mount

	
	ER or PBUR: Medcab-14.5 x 28.5
	12” to 14 1/2”
	16” to 27 1/2”
	Medcab

	
	FLEX: OM-Contour
	17 5/8”
	20” to 2”
	Outside Mount

	
	FLEX: Medcab-14.5 x 28.5
	12” to 14 1/2”
	20” to 27 1/2”
	Medcab

	Custom Panel Measurements – for best results, include picture of existing receptacle. Contact GPMS with questions.

	Quantity
	Width: Inside - Outside
	Height
	Depth
	Panel Type – OM, IN or MEDCAB

	
	-
	
	
	

	
	-
	
	
	



· Forward order form along with enMotion Sublease/End User Lease to:
installs@gapacms.com or fax to 877-329-4767 – for best results, forward a digital picture of the existing receptacle.
· Custom filler panels ship within 5-7 business days of receipt of order/lease.
· Video of Inner Mount filler panel installation: https://www.youtube.com/watch?v=G0Y9mAqsJjU
· Video of Outer Mount filler panel installation:  https://youtu.be/nTnhl-FAqVs
· Contact the GPMS Installation Team at 877-377-2737 with any questions. Thank you.
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